/******************** (C) COPYRIGHT 2008 STMicroelectronics ********************
* File Name          : readme.txt
* Author             : MCD Application Team
* Version            : V2.0.3
* Date               : 09/22/2008
* Description        : Description of the GPIO IOToggle Example.
********************************************************************************
* THE PRESENT FIRMWARE WHICH IS FOR GUIDANCE ONLY AIMS AT PROVIDING CUSTOMERS
* WITH CODING INFORMATION REGARDING THEIR PRODUCTS IN ORDER FOR THEM TO SAVE TIME.
* AS A RESULT, STMICROELECTRONICS SHALL NOT BE HELD LIABLE FOR ANY DIRECT,
* INDIRECT OR CONSEQUENTIAL DAMAGES WITH RESPECT TO ANY CLAIMS ARISING FROM THE
* CONTENT OF SUCH FIRMWARE AND/OR THE USE MADE BY CUSTOMERS OF THE CODING
* INFORMATION CONTAINED HEREIN IN CONNECTION WITH THEIR PRODUCTS.
*******************************************************************************/

Example description
===================
This example describes how to use GPIO BSRR (Port bit set/reset register) and 
BRR (Port bit reset register) for IO toggling.
These registers allow modifying only one or several GPIO pins in a single atomic
write access.
GPIO_LED Port Pin 6, Pin 7, Pin 8 and Pin 9 are toggled in an infinite loop.

Directory contents
==================
platform_config.h    Evaluation board specific configuration file
stm32f10x_conf.h     Library Configuration file
stm32f10x_it.c       Interrupt handlers
stm32f10x_it.h       Header for stm32f10x_it.c
main.c               Main program


Hardware environment
====================
This example runs on STMicroelectronics STM3210B-EVAL and STM3210E-EVAL evaluation
boards and can be easily tailored to any other hardware.
To select the STMicroelectronics evaluation board used to run the example, uncomment
the corresponding line in platform_config.h file.

 + STM3210B-EVAL 
    - Use LD1, LD2, LD3 and LD4 leds connected respectively to PC.06, PC.07, PC.08
      and PC.09 pins
 
 + STM3210E-EVAL
    - Use LD1, LD2, LD3 and LD4 leds connected respectively to PF.06, PF0.7, PF.08
      and PF.09 pins

    
How to use it
=============
In order to make the program work, you must do the following:
- Create a project and setup all your toolchain's start-up files
- Compile the directory content files and required Library files:
  + stm32f10x_lib.c
  + stm32f10x_gpio.c
  + stm32f10x_rcc.c
  + stm32f10x_nvic.c
  + stm32f10x_flash.c
  
- Link all compiled files and load your image into target memory
- Run the example


******************* (C) COPYRIGHT 2008 STMicroelectronics *****END OF FILE******
