The Dynamic Flash File System
•The dynamic flash file system allows the user to store data and web pages in the on-chip flash.
•NO RESET is requires to update the data.
•As a matter of fact, no local intervention at all is required.
•The update occurs over ethernet, using port 80, to easily get through many firewalls.
•The update can occur at anytime, the firmware automatically handles web page requests, while a update occurs.