MCF5223x

Thank you for Visiting the ColdFire Web Page.

Home Game

• V2 ColdFire core providing 48 Dhrystone @ 60 MHz executing out of on-chip Flash memory .
• Enhanced Multiply Accumulate Unit and hardware divide module
• Cryptographic Acceleration Unit coprocessor
• Fast Ethernet Controller
• On-chip Ethernet Transceiver
• FlexCAN controller area network module
• Three universal asynchronous/synchronous receiver/transmitters
• Inter-integrated circuit bus controller
• Queued serial peripheral interface module
• Eight-channel 12-bit fast analog-to-digital converter
• Four channel direct memory access controller
• Four 32-bit input capture/output compare timers with DMA support
• Four-channel general-purpose timer capable of input capture/output compare, pulse width modulation and pulse accumulation
• Eight/Four-channel 8/16-bit pulse width modulation timers (two adjacent 8-bit PWMs can be concatenated to form a single 16-bit timer)
• Two 16-bit periodic interrupt timers
• Real-time clock module
• Programmable software watchdog timer
• Two interrupt controllers providing every peripheral with a unique selectable-priority interrupt vector.
• Clock module and integrated phase locked loop
• Test access/debug port