Products Download Events Support |
Product Information Software & Hardware Products ARM Development Tools C166 Development Tools C51 Development Tools C251 Development Tools Debug Adapters Evaluation Boards Product Brochures Newsletters Device Database® Device List What is the Device Database? Why isn't a Device Listed? Adding to the Device Database Searching the Device Database Search by Architecture Search by Vendor Problem Report Feedback Downloads Product Download Compliance Testing ISO/ANSI Compliance Validation and Verification Distributors Overview | # STMicroelectronics STM32F103RB The STMicroelectronics STM32F103RB is an ARM 32-bit Cortex-M3 Microcontroller, 72MHz, 128kB Flash, 20kB SRAM, PLL, Embedded Internal RC 8MHz and 32kHz, Real-Time Clock, Nested Interrupt Controller, Power Saving Modes, JTAG and SWD, 3 Synch. 16-bit Timers with Input Capture, Output Compare and PWM, 16-bit 6-ch Advanced Timer, 2 16-bit Watchdog Timers, SysTick Timer, 2 SPI, 2 I2C, 3 USART, USB 2.0 Full Speed Interface, CAN 2.0B Active, 2 12-bit 16-ch A/D Converter, Fast I/O Ports.
| [Distributors]
Development Tools Compiler, Assembler, Linker, Debugger MDK-ARM (Microcontroller Development Kit) Keil MDK-Lite Download Keil
Evaluation Boards MCBSTM32 Keil 04. nanoMODUL-STM32F103 System on Module (SOM) Phytec iNEMO Demonstration board based on MEMS sensors and the STM32 STMicroelectronics
JTAG Debuggers ULINK-ME Keil ULINK2 Keil ULINKPro Keil J-Link ARM SEGGER Microcontroller
Data Sheets
Generic User Guide 1,364,135 bytes
Reference Manual 8,795,301 bytes
Technical Reference Manual 2,247,922 bytes
Application Notes STM32 Application Notes STMicroelectronics
Header Files STM32F10X.H 633,941 bytes
Example Code RL-ARM SD/MMC File Demo for MCBSTM32
Emulators Tanto ARM Hitex
FLASH Utilities FLASHit hse Electronic ULINK-ME Keil ULINK2 Keil ULINKPro Keil J-Link ARM SEGGER Microcontroller
Device Programmers Dataman 48Pro2 Super Fast Universal ISP Programmer Dataman Programmers Ltd. Dataman 48Pro2C Super Fast Universal ISP Programmer Dataman Programmers Ltd. Dataman 848Pro2 Super Fast Stand-Alone Programmer Dataman Programmers Ltd.
MDK Middleware The following middleware components are pre-configured in MDK-Professional CAN Driver Keil Flash File System Keil USB Device Interface Keil
Real-Time OS RTX Real-Time Operating System Keil
Simulated Features
NOTE Simulation for this device is provided by the default peripheral simulation driver. Complete peripheral simulation is not available and is not planned to be implemented by ARM.
The following on-chip peripherals are simulated by the Keil Software µVision Debugger. Alternate Function Input/Output (AFIO) Analog/Digital Converter 1 (ADC1) APB Bridge 1 APB Bridge 2 Backup Registers (BKP) DMA Controller (DMA) External Interrupts (EXTI) Fault Reports GPIO Port A - 16-Bit I/O GPIO Port B - 8-Bit I/O GPIO Port D - 2-Bit I/O I2C Interface Nested Vectored Interrupt Controller (NVIC) Power, Reset and Clock Control (PRCC) Real-Time Clock (RTC) Serial Peripheral Interface (SPI) System Control and Configuration System Tick Timer Timer 2 Timer 3 USART 1 USART 2 Watchdog - Independent Watchdog - Window
#### Products ##### Development Tools ARM C166 C51 C251 µVision IDE and Debugger | #### ##### Hardware & Collateral ULINK Debug Adaptors Evaluation Boards Product Brochures Device Database Distributors | #### Downloads MDK-ARM C51 C166 C251 File downloads | #### Support Knowledgebase Discussion Forum Product Manuals Application Notes | #### Contact Distributors Request a Quote Sales Contacts
| Cookie Settings | Terms of Use | Privacy | Accessibility | Contact Us | Feedback Copyright © 2005-2016 ARM Group. All rights reserved. |

##### Important information

This site uses cookies to store information on your computer. By continuing to use our site, you consent to our cookies.

Change Settings

/dd/chipinfo.asp