/**
  @page FLASH_Program FLASH_Program
  
  @verbatim
  ******************** (C) COPYRIGHT 2010 STMicroelectronics *******************
  * @file    FLASH/Program/readme.txt 
  * @author  MCD Application Team
  * @version V3.2.0
  * @date    03/01/2010
  * @brief   Description of the FLASH Program Example.
  ******************************************************************************
  * THE PRESENT FIRMWARE WHICH IS FOR GUIDANCE ONLY AIMS AT PROVIDING CUSTOMERS
  * WITH CODING INFORMATION REGARDING THEIR PRODUCTS IN ORDER FOR THEM TO SAVE
  * TIME. AS A RESULT, STMICROELECTRONICS SHALL NOT BE HELD LIABLE FOR ANY
  * DIRECT, INDIRECT OR CONSEQUENTIAL DAMAGES WITH RESPECT TO ANY CLAIMS ARISING
  * FROM THE CONTENT OF SUCH FIRMWARE AND/OR THE USE MADE BY CUSTOMERS OF THE
  * CODING INFORMATION CONTAINED HEREIN IN CONNECTION WITH THEIR PRODUCTS.
  ******************************************************************************
   @endverbatim

@par Example Description 

This example provides a description of how to program the STM32F10x FLASH.

After Reset, the Flash memory Program/Erase Controller is locked. To unlock it,
the FLASH_Unlock function is used.
Before programming the desired addresses, an erase operation is performed using 
the flash erase page feature. The erase procedure starts with the calculation of
the number of pages to be used. Then all these pages will be erased one by one by
calling FLASH_ErasePage function. 

Once this operation is finished, the programming operation will be performed by 
using the FLASH_ProgramWord function. The written data is then checked and the
result of the programming operation is stored into the MemoryProgramStatus variable.

@par Directory contents 

  - FLASH/Program/stm32f10x_conf.h   Library Configuration file
  - FLASH/Program/stm32f10x_it.h     Interrupt handlers header file
  - FLASH/Program/stm32f10x_it.c     Interrupt handlers
  - FLASH/Program/main.c             Main program

@par Hardware and Software environment 

  - This example runs on STM32F10x Connectivity line, High-Density, Medium-Density, 
    Medium-Density Value line, Low-Density and Low-Density Value line Devices.
  
  - This example has been tested with STMicroelectronics STM32100B-EVAL 
    (STM32F10x Medium-Density Value line), STM3210C-EVAL (STM32F10x Connectivity 
    line), STM3210E-EVAL (STM32F10x High-Density) and STM3210B-EVAL (STM32F10x 
    Medium-Density) evaluation boards and can be easily tailored to any 
    other supported device and development board. 
 
@par How to use it ? 

In order to make the program work, you must do the following:
- Create a project and setup all project configuration
- Add the required Library files:
  - stm32f10x_flash.c
  - system_stm32f10x.c (under Libraries\CMSIS\CM3\DeviceSupport\ST\STM32F10x) 
  
- Edit stm32f10x.h file to select the device you are working on.
  
@b Tip: You can tailor the provided project template to run this example, for 
        more details please refer to "stm32f10x_stdperiph_lib_um.chm" user 
        manual; select "Peripheral Examples" then follow the instructions 
        provided in "How to proceed" section.   
- Link all compiled files and load your image into target memory
- Run the example

@note
 - Low-density Value line devices are STM32F100xx microcontrollers where the 
   Flash memory density ranges between 16 and 32 Kbytes.
 - Low-density devices are STM32F101xx, STM32F102xx and STM32F103xx 
   microcontrollers where the Flash memory density ranges between 16 and 32 Kbytes.
 - Medium-density Value line devices are STM32F100xx microcontrollers where
   the Flash memory density ranges between 64 and 128 Kbytes.  
 - Medium-density devices are STM32F101xx, STM32F102xx and STM32F103xx 
   microcontrollers where the Flash memory density ranges between 64 and 128 Kbytes.
 - High-density devices are STM32F101xx and STM32F103xx microcontrollers where
   the Flash memory density ranges between 256 and 512 Kbytes.
 - Connectivity line devices are STM32F105xx and STM32F107xx microcontrollers.  
   
 * <h3><center>&copy; COPYRIGHT 2010 STMicroelectronics</center></h3>
 */
