Back to Release page
# Release Notes for STM32F10x Standard Peripherals Library Examples (StdPeriph_Examples) Copyright 2010 STMicroelectronics
## Contents STM32F10x Standard Peripherals Library Examples update History License ## STM32F10x Standard Peripherals Library Examples update History ### 3.2.0 - 03/01/2010 General Add support for STM32 Low-density Value line (STM32F100x4/6) and Medium-density Value line (STM32F100x8/B) devices for almost examples. Add new examples: HDMI-CEC, Dual CAN, PVD and TIM15 Complementary Signals. STM32F10x_StdPeriph_Examples CAN Add new example Dual CAN: This example shows how to configure the CAN1 and CAN2 peripherals to send and receive CAN frames in normal mode. The sent frames are used to control Leds by presseing KEY or Tamper push buttons. CAN Normal example renamed to CAN Networking example. CEC New example: This example provides a basic communication between two HDMI-CEC devices using interrupts. PWR New example PVD: This example shows how to configure the programmable voltage detector using an external interrupt line. TIM New example TIM15 Complementary Signals: This example shows how to configure the TIM15 peripheral to generate one complementary TIM15 signal, to insert a defined dead time value, to use the break feature and to lock the desired parameters. Cascade_Synchro,Parallel_Synchro, ExtTrigger_Synchro, TIM1_Synchro examples main files: Add TIM_SelectMasterSlaveMode() function call for all slaves and masters. I2C EEPROM example: the i2c_ee.h/.c files are removed. The example is using the new Serial EEPROM driver stm32_eval_i2c_ee.h/.c driver available under Utilities\STM32_EVAL\Common. SPI M25P64_FLASH example renamed to SPI_FLASH: the spi_flash.h/.c files are removed. The example is using the new Serial SPI FLASH driver stm32_eval_spi_flash.h/.c driver available under Utilities\STM32_EVAL\Common. SDIO The sdcard.h/.c files are removed. The example is using the new SD Card driver stm32_eval_sdio_sd.h/.c driver available under Utilities\STM32_EVAL\Common. FSMC All FSMC example: the fsmc_sram.h/.c, fsmc_nor.h/.c and fsmc_nand.h/.c files are removed. The examples are using the new FSMC memories drivers stm3210e_eval_fsmc_sram.h/.c, stm3210e_eval_fsmc_nor.h/.c and stm3210e_eval_fsmc_nand.h/.c drivers available under Utilities\STM32_EVAL\STM3210E_EVAL. DMA FSMC example: the fsmc_sram.h/.c files are removed. The example is using the new FSMC SRAM driver stm3210e_eval_fsmc_sram.h/.c driver available under Utilities\STM32_EVAL\STM3210E_EVAL. ADC All ADC examples are using a dedicated system_stm32f10x.c file to configure the system core clock to 56MHz. ## License The enclosed firmware and all the related documentation are not covered by a License Agreement, if you need such License you can contact your local STMicroelectronics office. THE PRESENT FIRMWARE WHICH IS FOR GUIDANCE ONLY AIMS AT PROVIDING CUSTOMERS WITH CODING INFORMATION REGARDING THEIR PRODUCTS IN ORDER FOR THEM TO SAVE TIME. AS A RESULT, STMICROELECTRONICS SHALL NOT BE HELD LIABLE FOR ANY DIRECT, INDIRECT OR CONSEQUENTIAL DAMAGES WITH RESPECT TO ANY CLAIMS ARISING FROM THE CONTENT OF SUCH FIRMWARE AND/OR THE USE MADE BY CUSTOMERS OF THE CODING INFORMATION CONTAINED HEREIN IN CONNECTION WITH THEIR PRODUCTS. For complete documentation on STM32(CORTEX M3) 32-Bit Microcontrollers visit www.st.com/STM32