/******************** (C) COPYRIGHT 2008 STMicroelectronics ********************
* File Name          : readme.txt
* Author             : MCD Application Team
* Version            : V2.0.3
* Date               : 09/22/2008
* Description        : Description of the FSMC NAND Example.
********************************************************************************
* THE PRESENT FIRMWARE WHICH IS FOR GUIDANCE ONLY AIMS AT PROVIDING CUSTOMERS
* WITH CODING INFORMATION REGARDING THEIR PRODUCTS IN ORDER FOR THEM TO SAVE TIME.
* AS A RESULT, STMICROELECTRONICS SHALL NOT BE HELD LIABLE FOR ANY DIRECT,
* INDIRECT OR CONSEQUENTIAL DAMAGES WITH RESPECT TO ANY CLAIMS ARISING FROM THE
* CONTENT OF SUCH FIRMWARE AND/OR THE USE MADE BY CUSTOMERS OF THE CODING
* INFORMATION CONTAINED HEREIN IN CONNECTION WITH THEIR PRODUCTS.
*******************************************************************************/

Example description
===================
This example provides a basic example of how to use the FSMC firmware library and
an associate driver to perform erase/read/write operations on the NAND512W3A2 memory
mounted on STM3210E-EVAL board.


Directory contents
==================
stm32f10x_conf.h    Library Configuration file
stm32f10x_it.c      Interrupt handlers
stm32f10x_it.h      Header for stm32f10x_it.c
fsmc_nand.c         Driver for NAND memory
fsmc_nand.h         Header for fsmc_nand.c 
main.c              Main program


Hardware environment
====================
This example runs on STMicroelectronics STM3210E-EVAL evaluation board RevD.

Note: make sure that the Jumper 7 (JP7) is in position 1<-->2. 

    
How to use it
=============
In order to make the program work, you must do the following:
- Create a project and setup all your toolchain's start-up files
- Compile the directory content files and required Library files:
  + stm32f10x_lib.c
  + stm32f10x_gpio.c
  + stm32f10x_rcc.c
  + stm32f10x_nvic.c
  + stm32f10x_flash.c
  + stm32f10x_fsmc.c
  
- Link all compiled files and load your image into target memory
- Run the example


******************* (C) COPYRIGHT 2008 STMicroelectronics *****END OF FILE******
