Products Download Events Support |
Product Information Product Overview Supported Microcontrollers Shows and Seminars Technical Support Support Knowledgebase Product Manuals Application Notes Discussion Forum Software Downloads Product Downloads File Downloads Other Information Books Links Contact Information Corporate Sales Channels Distributors | # STMicroelectronics STM32F102C8 ARM Cortex-M3, 48 MHz, 10 kB RAM, 64 kB ROM STMicroelectronics' STM32F1 series of mainstream MCUs covers the needs of a large variety of applications in the industrial, medical and consumer markets. High performance with first-class peripherals and low-power, low-voltage operation is paired with a high level of integration at accessible prices with a simple architecture and easy-to-use tools. Typical applications include motor drives and application control, medical and handheld equipment, industrial applications, PLCs, inverters, printers, and scanners, alarm systems, video intercom, HVAC and home audio equipment. - LCD parallel interface, 8080/6800 modes - 5 V-tolerant I/Os - Timer with quadrature (incremental) encoder input - 96-bit unique ID Core ARM Cortex-M3 48 MHz Processor:ARM Cortex-M3, 48 MHz Timer/Counter/PWM 3 x 16-bit Timer Watchdog:2 x Watchdog Timer/Counter:3 x 16-bit Timer/Counter Module Clock & Power 2.00 V .. 3.60 V, 48 MHz RTC:32 kHz RTC Supply Voltage:2.00 V .. 3.60 V Operating Voltage Maximum Clock Frequency:48 MHz I/O & Package -40 °C .. 85 °C, -40 °C .. 105 °C, 48-QFP Operating Temperature Range:-40 °C .. 85 °C Operating Temperature Range Operating Temperature Range:-40 °C .. 105 °C Operating Temperature Range I/Os:36 Inputs/Outputs Package, QFP:48-lead QFP Communication USB, Device, SPI, I2C, USART USB, Device:1 x USB Device SPI:2 x 12 Mbit/s SPI I2C:2 x I2C USART:3 x 4 Mbit/s USART Analog 10-channel 16-bit ADC ADC:10-channel x 16-bit ADC Memory 10 kB RAM, 64 kB ROM ROM:64 kB RAM:10 kB Quick Links Board List Software Packs MDK Version 5 Legacy Support Feedback Silicon Supplier STMicroelectronics Device Family Pack DFP Support for this device is contained in: STMicroelectronics STM32F1 Series Device Support, Drivers and Examples Download
Development Tools | MDK Version 5 (Microcontroller Development Kit) MDK-Lite Download
CMSIS Drivers | CAN Driver for STM32F1 Series Ethernet MAC Driver for STM32F1 Series I2C Driver for STM32F1 Series MCI Driver for STM32F1 Series SPI Driver for STM32F1 Series UART Driver for STM32F1 Series USB Device Driver for STM32F1 Connectivity Line Devices USB Device Driver for STM32F1 Series USB Host Driver for STM32F1 Connectivity Line Devices
Examples | CMSIS-RTOS Blinky MCBSTM32C Demo MCBSTM32C emWin Example MCBSTM32C emWin GUI Demo MCBSTM32C CAN Data MCBSTM32C CAN RTR MCBSTM32C USB Device HID MCBSTM32C USB Device Mass Storage MCBSTM32C USB Device Virtual COM MCBSTM32C USB Host Mass Storage MCBSTM32C USB Host Keyboard MCBSTM32C File System Demo MCBSTM32C BSD Client MCBSTM32C BSD Server MCBSTM32C FTP Server MCBSTM32C HTTP Server MCBSTM32C SMTP Client MCBSTM32C SNMP Agent MCBSTM32C Telnet Server MCBSTM32C CMSIS-RTOS Blinky MCBSTM32E emWin Example MCBSTM32E emWin GUI Demo MCBSTM32E CAN Data MCBSTM32E CAN RTR MCBSTM32E USB Device HID MCBSTM32E USB Device Mass Storage MCBSTM32E USB Device Virtual COM MCBSTM32E File System Demo MCBSTM32E
### End User Licence Agreement (EULA) Do you Accept or Decline the terms of this License Agreement?
#### Products ##### Development Tools ARM C166 C51 C251 µVision IDE and Debugger | #### ##### Hardware & Collateral ULINK Debug Adaptors Evaluation Boards Product Brochures Device Database Distributors | #### Downloads MDK-ARM C51 C166 C251 File downloads | #### Support Knowledgebase Discussion Forum Product Manuals Application Notes | #### Contact Distributors Request a Quote Sales Contacts
| Cookie Settings | Terms of Use | Privacy | Accessibility | Contact Us | Feedback Copyright © 2005-2016 ARM Group. All rights reserved. |

##### Important information

This site uses cookies to store information on your computer. By continuing to use our site, you consent to our cookies.

Change Settings