DOWNLOAD.EXE: ADuC program downloader ver  2.07 (NT compatible - modified by Kem
t FEI TU Kosice, May, 2003)
18th Oct, 1999 C.King Accutron Ltd.

Program options:

  a filename must be specified on the command line
  /C:n    select the com port (default is 1)
  /F:n.n  select the target crystal freq in MHz (default 11.0592)
  /D      do not erase Flash/EE data space (firmware rev 2.0 or greater)
  /R      run the program from the beginning (0000 hex)
  /R:xxxx run the program from the specified start address

Example:

  DOWNLOAD filename.hex /c:1 /f:16 /d /r
